# Gloss Interpretation

## Gloss Values and Their Meaning

Gloss is measured in Gloss Units (GU). Here are some typical gloss values for different materials:


| Material             | 60-Degree Gloss Value |
|:---------------------|:----------------------|
| Automotive Clearcoat | 85-95 GU              |
| Semi-Gloss Paint     | 50-75 GU              |
| Satin Paint          | 25-35 GU              |
| Matte Paint          | 5-15 GU               |
| Polished Metals      | 300-950 GU            |
| Perfect Mirror       | 1000 GU               |

Higher values indicate a more reflective, glossier surface.

## Visualizing Gloss in Appearance Elements


## Changing Surface Gloss

To change the gloss of a surface:

1. **Surface Texture**: Smoother surfaces generally have higher gloss. Polishing or sanding can increase gloss, while roughening the surface can decrease it.
2. **Coating Formulation**: For coated surfaces, adjust the refractive index of the coating. Higher refractive index materials tend to be glossier.
3. **Pigmentation**: For paints, the type and amount of pigments can affect gloss. Generally, fewer pigments result in higher gloss.
4. **Application Method**: The way a coating is applied can impact gloss. Spray application often yields higher gloss than brush application.
5. **Curing Conditions**: For certain coatings, the curing process can affect final gloss. Proper curing conditions are essential for achieving desired gloss levels.
6. **Substrate**: The underlying material can influence gloss. A smoother substrate often results in a glossier finish.

Remember that changing gloss may affect other surface properties, so consider the overall impact on the product's performance and appearance.
