# Visual Haze Interpretation

| Haze                       | Surface                | Description/Perception                                                    |
|----------------------------|------------------------|---------------------------------------------------------------------------|
| <50 Hu (Indoor or outdoor) | High Quality Surface   | Almost perfect surface- haze not visible under normal viewing conditions. |
| 50-100                     | Ultra Low Haze Surface | Good depth of finish- Barely visible halo around reflected light sources. |
| 100-250                    | Visible Haze           | Depth of finish is compromised- swirls and polishing marks are visible    |
| 250-300                    | Hazy Surface           | Poor quality finish                                                       |
| 300-500                    | Poor Quality Surface   | Prominent halos, holograms or polish marks. Poor depth of finish          |

