# Visual Demo Module
This module is used to manually control Aesthetix light sources and cameras. Surface or gloss images from these screens can be saved with or without overlays.


# Surface View Mode
![Visual Demo screen](Visual Demo.png)



## Surface View Controls
1. 45 Degree Light- toggle between all on and all off.
2. Overlay control- switch on overlays to indicate measurement areas for Aesthetix Modules.
3. Camera exposure control, click "A" to activate auto-exposure or use manual slider.
4. Individual LED control (Line light, 6 x 45 degree ring lights, 10 degree spotlight )
5. Image Controls (Reset view, switch to gloss view, reset camera, copy image to clipboard, save image to file)

![Visual demo specular camera](visual demo specular.png)

# Gloss View Mode

6. Specular 60 degree light toggle on/off.
7. Camera exposure control, click "A" to activate auto-exposure or use manual slider.
8. Image Controls (Reset view, switch to surface view, reset camera, copy image to clipboard, save image to file).
9. Toggle gloss overlay.